{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["litho","Hydro","Formtation"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"litho","index":0,"n_rows":36,"n_cols":2,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[null,"W-6182                         "]
[null,"                                         Lithologic Details                                         "]
[null,"                                         ==================                                         "]
[null,"Station                        X-Coord. Y-Coord."]
[null,"                                (feet)   (feet) "]
[null,"------------------------------ -------- --------"]
[null,"W-6182                         493367   1355872 "]
[null," "]
[null,"Min. Depth Max. Depth Primary Rock                   % Primary Rock         Primary Color                    Induration           % Porosity                      Comments                     "]
[null,"---------- ---------- ------------------------------ -------------- ------------------------------ ------------------------------ ---------- --------------------------------------------------"]
[null,"0          30         NO SAMPLE                                                                                                                                                                "]
[null,"30         40         SAND (QUARTZ)                                                                UNCONSOLIDATED                 34                                                           "]
[null,"40         50         CLAY                                                                         MODERATE                       12                                                           "]
[null,"50         130        NO SAMPLE                                                                                                                                                                "]
[null,"130        140        SAND (QUARTZ)                                                                UNCONSOLIDATED                 34                                                           "]
[null,"140        150        SAND (QUARTZ)                                                                UNCONSOLIDATED                 35                                                           "]
[null,"150        160        NO SAMPLE                                                                                                                                                                "]
[null,"160        170        SAND (QUARTZ)                                 VERY LIGHT ORANGE              UNCONSOLIDATED                 34                                                           "]
[null,"170        180        CLAY                                                                         MODERATE                       12                                                           "]
[null,"180        190        CLAY                                                                         MODERATE                       20                                                           "]
[null,"190        200        LIMESTONE                                                                    GOOD                           20                                                           "]
[null,"200        210        LIMESTONE                                     BLACK                          GOOD                           20                                                           "]
[null,"210        220        LIMESTONE                                     BLACK                          GOOD                           20                                                           "]
[null,"220        240        LIMESTONE                                                                                                                                                                "]
[null,"240        250        CALCARENITE                                                                  UNCONSOLIDATED                 30         WITH LEPS AND OPERCULINOIDES SP.                  "]
[null,"250        260        CALCARENITE                                                                  UNCONSOLIDATED                 30                                                           "]
[null,"260        270        CALCARENITE                                                                  UNCONSOLIDATED                 30         WITH GYPSINA GLOBULA WITH ALABAMINA OBTUSA WITH AM"]
[null,"                                                                                                                                             PHISTIGIMA PINNARENSIS DISCORINOPSIS GUNTERI, DICT"]
[null,"                                                                                                                                             YCONUS COOKEI, SPIROLINA CORYENSIS ABOVE FOSSILS A"]
[null,"                                                                                                                                             PPEAR REWORKED AND BROKEN                         "]
[null,"270        620        CALCARENITE                                                                                                                                                              "]
[]
[null,"Main Menu |"]

{"sheet":"Hydro","index":1,"n_rows":13,"n_cols":1,"rows_kept":13,"cut":false,"hidden":false,"merged":[]}
[]
[]
["                        Hydrostratigraphy Details                            "]
["                           =========================                            "]
[]
["Station                        X-Coord. Y-Coord."]
["                                (feet)   (feet) "]
["------------------------------ -------- --------"]
["W-6182                         493367   1355872 "]
[" "]
["Min. Depth Max. Depth Aquifer                        Aquifer Source                 Aquifer Source Reference                          "]
["---------- ---------- ------------------------------ ------------------------------ --------------------------------------------------"]
["40                    INTERMEDIATE CONFINING UNIT    FLORIDA GEOLOGICAL SURVEY      Arthur, J. etal, 2005: FGS Bulletin 68            "]

{"sheet":"Formtation","index":2,"n_rows":31,"n_cols":1,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
[]
["                           Formation Details                                "]
["                               =================                                "]
[]
["Station                        X-Coord. Y-Coord."]
["                                (feet)   (feet) "]
["------------------------------ -------- --------"]
["W-6182                         493367   1355872 "]
[" "]
["Min. Depth Max. Depth Formation                      Formation Source               Formation Source Reference                        "]
["---------- ---------- ------------------------------ ------------------------------ --------------------------------------------------"]
["0          190        Undifferentiated sand and clay FLORIDA GEOLOGICAL SURVEY                                                        "]
["40                    Peace River Formation          FLORIDA GEOLOGICAL SURVEY      2003 INTERIM                                      "]
["190        250        Hawthorn Group                 FLORIDA GEOLOGICAL SURVEY                                                        "]
["250        310        Crystal River Formation        FLORIDA GEOLOGICAL SURVEY                                                        "]
["310        340        Ocala Limestone Lower Member   FLORIDA GEOLOGICAL SURVEY                                                        "]
["340        620        Avon Park Formation            FLORIDA GEOLOGICAL SURVEY                                                        "]
[]
[]
[]
["                                 Formation Age                                  "]
["                               =================                                "]
[]
["Station              Min. Depth Max. Depth Formation Age Type                                 Elev From  Elev To    Formation Age Source           Formation Age Source Reference                    "]
["-------------------- ---------- ---------- -------------------------------------------------- ---------- ---------- ------------------------------ --------------------------------------------------"]
["W-6182               0          190        Undifferentiated                                   105        -85                                                                                         "]
["W-6182               190        250        Miocene                                            -85        -145                                                                                        "]
["W-6182               250        620        Eocene                                             -145       -515                                                                                        "]